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Safety Data Sheet

1 – Product Identifier & Identity for the Chemical
	Manufacturer:	WD-40 Company Australia          Pty Ltd

Address:	41 Rawson Street 
     (Level 2, Suite 23)
	 	Epping
		NSW, 2121, Australia
Telephone:  
Information: +61 2 9868 2200
Emergency only: 1800 862 115 

Poisons Information Centre: 
Australia: 13 11 26
New Zealand: 0800 764 766

New Zealand Contact Details:
Name:               Eproducts New Zealand Limited
Address:          1B / 89 Ellice Road,
Wairau Valley,
Auckland 0629
New Zealand
Telephone
Information: 09 916 6750
Emergency only: 0800 425 459
	Product Name: WD-40 Non-Aerosol Trigger Spray

Chemical Name: Mixture

Product Use: Lubricant, Penetrant, Drives Out Moisture, Removes and Protects Surfaces From Corrosion

Restriction on Use: None Identified

SDS Date Of Preparation: 21 May 2026

This SDS applies to unit codes: 62101




2 – Hazards Identification

Classification of the Hazardous Chemical (in accordance with WHS Regulation)

	Health
	Environmental
	Physical

	Aspiration Toxicity Category 1
	Not Hazardous
	Flammable Liquid Category 4



Label Elements 
[image: ]
Contains: Distillates (petroleum), hydrotreated light

Danger!
H227 Combustible liquid.
H304 May be fatal if swallowed and enters airways. 
AUH066 Repeated exposure may cause skin dryness or cracking.

Prevention
P210 Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking. 
P280 Wear protective gloves.
Response
P301+P310 IF SWALLOWED: Immediately call a POISON CENTER or doctor. 
P331 Do NOT induce vomiting. 
P370+P378 In case of fire: Use water fog, dry chemical, carbon dioxide or foam to extinguish.  
Storage
P403 Store in a well-ventilated place. 
P405 Store locked up. 
Disposal
P501 Dispose of contents and container in accordance with local and national regulations. 

Other Hazards that do not Result in Classification: None

3 - Composition/Information on Ingredients
	Ingredient
	CAS #
	Weight Percent
	Substance Classification

	Distillates (petroleum), hydrotreated light
	64742-47-8
	50-70%
	Flam. Liq. Cat 4 (H227)
Asp. Tox. Cat 1 (H304)
AUH066

	Petroleum Base Oils
	Mixture
	10-<30%
	Not Hazardous 


See Section 16 for full text of GHS Classification and H phrases

4 – First Aid Measures
Ingestion (Swallowed): Aspiration Hazard. DO NOT induce vomiting. Call a Poisons Information Center (phone 13 11 26 from anywhere in Australia or 0800 764 766 in New Zealand) immediately. 
Eye Contact: Flush thoroughly with water. Remove contact lenses if present after the first 5 minutes and continue flushing for several more minutes. Get medical attention if irritation persists.
Skin Contact: Wash with soap and water. If irritation develops and persists, get medical attention.
Inhalation (Breathing): If irritation is experienced, move to fresh air. Get medical attention if irritation or other symptoms develop and persist.
Most Important Symptoms: Harmful or fatal if swallowed. Accidental ingestion may cause gastrointestinal effects with irritation, nausea, vomiting, dizziness, coma and death. Aspiration into the lungs during ingestion or vomiting may cause lung damage. May cause eye irritation. Skin contact may cause drying of the skin. Inhalation of mists may cause coughing, headache and dizziness. 
Indication of Immediate Medical Attention and Special Treatment, if Needed: Immediate medical attention is required for ingestion.

5 – Fire Fighting Measures
Suitable Extinguishing Media: Use water fog, dry chemical, carbon dioxide or foam. Do not use water jet or flooding amounts of water. Burning product will float on the surface and spread fire.
Specific Hazards Arising from the Chemical: Combustible liquid. Vapors are heavier than air and may travel along surfaces to remote ignition sources and flash back. A vapor and air mixture can create an explosion hazard in confined spaces. Combustion will produce oxides of carbon and hydrocarbons. 
Special Protective Equipment and Precautions for Fire-Fighters: Firefighters should always wear positive pressure self-contained breathing apparatus and full protective clothing. Cool fire-exposed containers with water.

6 – Accidental Release Measures
Personal Precautions, Protective Equipment and Emergency Procedures: Eliminate all sources of ignition and ventilate area. Wear appropriate protective clothing (see Section 8). Environmental Precautions: Report spills to authorities as required.
Methods and Materials for Containment/Cleanup: Contain and collect liquid with an inert absorbent material and place in a container for disposal. Clean spill area thoroughly. 

7 – Handling and Storage
Precautions for Safe Handling: Avoid contact with eyes. Avoid prolonged contact with skin. Avoid breathing vapors or mists. Use only with adequate ventilation. Keep away from heat, sparks, hot surfaces and open flames. Wash thoroughly with soap and water after handling. Keep containers closed when not in use. Keep out of the reach of children.
Conditions for Safe Storage, including any incompatibilities: Store in a cool, dry ventilated area away from incompatible materials.

8 – Exposure Controls /Personal Protection
	Chemical
	Occupational Exposure Limits
	Biological Limit Value

	Distillates (petroleum), hydrotreated light
	1200 mg/m3 TWA (manufacturer recommended)
	None Established

	Petroleum Base Oils
	5 mg/m3 TWA AU OEL (as oil mist, refined mineral)
5 mg/m3 TWA, 10 mg/m3 STEL NZ OEL (as oil mist, mineral)
5 mg/m3 TWA ACGIH TLV (inhalable) (as mineral oil)
	None Established



The Following Controls are Recommended for Normal Consumer Use of this Product
Appropriate Engineering Controls: Use in a well-ventilated area.
Personal Protection:
Eye Protection: Avoid eye contact. Safety glasses or goggles recommended.
Skin Protection: Avoid prolonged skin contact. Chemical resistant gloves recommended for operations where skin contact is likely.
Respiratory Protection: None needed for normal use with adequate ventilation.

For Bulk Processing or Workplace Use the Following Controls are Recommended
Appropriate Engineering Controls: Use adequate general and local exhaust ventilation to maintain exposure levels below that occupational exposure limits.
Personal Protection: 
Eye Protection: Safety goggles recommended where eye contact is possible.
Skin Protection: Wear chemical resistant gloves. 
Respiratory Protection: None required if ventilation is adequate. If the occupational exposure limits are exceeded, wear an approved respirator. Respirator selection and use should be based on contaminant type, form and concentration. Follow applicable regulations and good Industrial Hygiene practice.
Work/Hygiene Practices: Wash with soap and water after handling.
Other Protective Equipment: None required. 

9 – Physical and Chemical Properties
	Appearance and Odor:
	Light amber liquid with a mild petroleum odor
	Partition Coefficient of n-octanol/water:
	Not established

	Odor Threshold:
	Not established
	Auto-ignition temperature:
	462.2°F (239°C)

	pH:
	Not established
	Decomposition Temperature:
	Not established

	Melting/Freezing Point:
	Not established

	Viscosity:
	3.72 mm2/sec @104°F (40°C)

	Boiling Point / Range: 
	 296.6-1225.4°F (147-663°C)
	Specific Heat Value:
	Not determined

	Flash Point:
	175°F (79.5°C) 
	Particle Size:
	Not determined

	Evaporation Rate 
(Butyl Acetate = 1): 
	Not determined
	VOC:
	65%

	Flammability (solid, gas):
	Not applicable
	Percent Volatile:
	Not determined

	Flammable Limits:
(Distillates (petroleum), hydrotreated light)  
	LEL: 0.6%  
UEL: 5.0%
	Saturated Vapor Concentration:
	Not determined

	Vapor Pressure: 
	0.023 kPa @ 68°F (20°C)
	Release of invisible flammable vapors and gases: 
	No

	Vapor Density (air = 1): 
	6.2
	Aerosol Protection Level (NFPA 30B):
	Not applicable

	Relative Density (Water = 1): 
	Not established
	Solubility:
	Insoluble in water



10 – Stability and Reactivity
Reactivity: Non-reactive
Chemical Stability: Stable under normal storage conditions.
Possibility of Hazardous Reactions: Hazardous polymerization will not occur.
Conditions to Avoid: Avoid heat, sparks, flames and other sources of ignition. 
Incompatible Materials: Strong oxidizing agents.
Hazardous Decomposition Products: Carbon monoxide, carbon dioxide, and hydrocarbons. 

11 – Toxicological Information
Health Hazards:
Ingestion: This product has low oral toxicity. Swallowing may cause gastrointestinal irritation, nausea, vomiting and diarrhea. This product is an aspiration hazard. If swallowed, can enter the lungs and may cause chemical pneumonitis, severe lung damage and death. 
Eye Contact: Contact may be irritating to eyes. May cause redness and tearing.
Skin Contact: Prolonged and/or repeated contact may produce mild irritation and defatting with possible dermatitis.
Inhalation: High concentrations may cause nasal and respiratory irritation and central nervous system effects such as headache, dizziness and nausea. Intentional abuse may be harmful or fatal.
Chronic Exposure: None expected.
Medical Conditions Aggravated by Exposure: Preexisting eye, skin and respiratory conditions may be aggravated by exposure.

Acute Toxicity Values:
Acute Toxicity Estimates: Oral > 5,000 mg/kg; Dermal >2,000 mg/kg based on an assessment of the ingredients. This product is not classified as toxic by established criteria.
ATEmix Oral: >2,000 mg/kg; Dermal: >2,000 mg/kg; Not acutely toxic by inhalation 

Skin Corrosion/Irritation: No data available for mixture. Based on the ingredients, this product is not classified as a skin irritant. 
Serious Eye Damage/Irritation: No data available for mixture. Based on the ingredients, this product is not classified as an eye irritant.
Respiratory or Skin Sensitization: This product is not expected to cause sensitization.
Germ Cell Mutagenicity: None of the components have been found to be mutagenic.
Carcinogenicity: None of the components are listed as a carcinogen or suspected carcinogen by IARC, NTP, ACGIH, US OSHA or the EU CLP.
Reproductive Toxicity: None of the components are known to cause adverse reproductive effects.
Specific Target Organ Toxicity:
	Single Exposure: No data available. 
	Repeated Exposure: No data available. 
Aspiration Hazard: Based on viscosity data this product is expected to present an aspiration hazard and may be harmful if the contents are swallowed. 

12 – Ecological Information
Ecotoxicity: No specific aquatic toxicity data is currently available; however components of this product are not expected to be harmful to aquatic organisms. If applied to leaves may kill grasses and small plants by interfering with respiration and transpiration. This product is not toxic to fish but may coat gill structures resulting in suffocation.
Persistence and Degradability: Components are readily biodegradable.
Bioaccumulative Potential: Bioaccumulation is not expected based on an assessment of the ingredients.
Mobility in Soil: No data available.
Other Adverse Effects: None Known

13 - Disposal Considerations
Safe Handling and Disposal Method: Dispose as appropriate for oil waste.
Disposal of Contaminated Packaging: Empty containers may be disposed of through normal waste management options.
Environmental Regulations: Dispose of all waste product, absorbents, and other materials in accordance with applicable Federal, state and local regulations.

14 – Transportation Information
IMDG Shipping Name: Not Regulated
IMDG Hazard Class: None
UN Number: None

IATA Shipping Name: Not Regulated
IATA Hazard Class: None
UN Number: None

ADG Shipping Name: Not Regulated
ADG Hazard Class: None
UN Number: None
Hazchem (Emergency Action) Code: None

Special Precautions for User: WD-40 Company does not test containers to assure that they can withstand the pressure change without leakage when transported by air. We do not recommend that our products be transported by air unless a specific review is conducted.

15 – Regulatory Information
Montreal Protocol (Ozone Depleting Substances): None present
The Stockholm Convention (Persistent Organic Pollutants): None present
The Rotterdam Convention (Prior Informed Consent): Not applicable
Basel Convention: Not applicable
International Convention for the Prevention of Pollution from Ships (MARPOL): Not applicable
Standard for the Uniform Scheduling of Medicines and Poisons (SUSMP): Hydrocarbons, liquids are listed in Schedule 5.

Australian Inventory of Chemical Substances: All of the components of this product are listed on the AICS inventory.

New Zealand:
HSNO Approval Number: HSR002602
Considered a Hazardous Substance according to the criteria of the New Zealand Hazardous Substances New Organisms legislation. Not classified as Dangerous Good for transport purposes. 

HSNO Hazard Classes: 3.1D, 6.1E

New Zealand Inventory: All the ingredients comply with the HSNO regulations.

16 – Other Information
REVISION DATE: 21 May 2026 			SUPERSEDES: 2 July 2021   	

Revision History:
21 May 2026: Updated address

Prepared By: Industrial Health & Safety Consultants, Inc.

Full Text of GHS Classification and H Phrases from Section 3:
Asp. Tox. Cat 1 Aspiration Toxicity Category 1
Flam. Liq. Cat 4 Flammable Liquid Category 4
H227 Combustible liquid
H304 May be fatal if swallowed and enters airways. 
AUH066 Repeated exposure may cause skin dryness or cracking.

List of Abbreviations or Acronyms:
ACGIH American Conference of Industrial Hygienists
ADG Australian Dangerous Goods
AICS Australian Inventory of Chemical Substances
AU Australia
EC Effective Concentration
EU European Union
GHS Globally Harmonized System of Classification and Labelling of Chemicals
HSNO Hazardous Substances and New Organisms 
IARC International Agency of Research on Cancer
IATA International Air Transport Association
IMDG International Maritime Dangerous Goods
LC Lethal Concentration
LD Lethal Dosage
LEL Lower Explosive Limit
NTP National Toxicology Program
NZ New Zealand
OEL Occupational Exposure Limits
PEL Permissible Exposure Limit
SDS Safety Data Sheet
STEL Short Term Exposure Limit
TWA Time-Weighted Average
UEL Upper Explosive Limit
US OSHA United States Occupational Safety and Health Administration
VOC Volatile Organic Compounds
WHS Work Health and Safety

REVIEWED BY:	I. Kowalski			TITLE:	Manager Regulatory Affairs	


This SDS complies with Australian guidelines for SDS. The foregoing information has been compiled from sources believed to be accurate but is not warranted to be. Recipients are advised to confirm in advance of need that data is correct. Standards change without notice. It is the responsibility of the recipient to insure that their personnel have been notified of any changes which may affect them. The data provided on this SDS are not meant to be used as specifications, only as guideline information as to the safe use of this product. User should refer to applicable laws before use.
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